|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Item** | **Product** | **Material** | **Hardness(HRC)** | **Diameter (mm)** | **Length (mm)** | **Head** | **Point** | **Surface Treatment** |
| Y-13A | washered steel nail | Steel | 54° ~ 57° | 3.7 | 25 ~ 75 | flat)  | needle | Zinc Plating |
| Y-13B | washered steel nail |  Steel |  54° ~ 57° |  3.7 | 25 ~ 75  |  flat | needle  |  Zinc Plating |
|  Y-13C |  washered steel nail |  Steel |  54° ~ 57° |  3.7 |  25 ~ 75 | flat |  needle |  Zinc Plating |
|  Y-13D |  washered steel nail |  Steel |  54° ~ 57° |  2.5~3.7 |  25 ~ 75 |  flat | needle |  Zinc Plating |
|  Y-13E |  washered steel nail |  Steel |  54° ~ 57° |  2.5~3.6 |  25 ~ 75 | flat |  needle |  Zinc Plating |